|  |  |  |  |
| --- | --- | --- | --- |
|  | **Name** | **Signature** | **Date** |
| **Prepared by:** | Vincent |  |  |
| **Reviewed by:** |  |  |  |
| **Approved by:** |  |  |  |



Doc name: 03-API-Z90 Contact IC Card Reader 1.00.docx

**Application Program Interface**

**1.00**

**Z90 Contact IC Card Reader**

# Version History

| **Date** | **By** | **Changes** | **Version** |
| --- | --- | --- | --- |
| 2016-09-22 | Vincent |  | 1.00 |
| 2016-10-08 | Vincent | Add the function of RF card | 1.10 |
|  |  |  |  |

Contents

[Version History 2](#_Toc458156288)

[1.0. Introduction 4](#_Toc458156289)

[2.0. Application Program Interface 5](#_Toc458156290)

[2.1. Device Function 5](#_Toc458156291)

[2.1.1. Initialize the port 5](#_Toc458156292)

[2.1.2. Close the port 5](#_Toc458156293)

[2.1.3. Beep 5](#_Toc458156294)

[2.1.4. RF reset 6](#_Toc458156295)

[2.1.5. Get the version of the hardware 6](#_Toc458156296)

[2.1.6. Exchange decimal character string into hexadecimal 6](#_Toc458156297)

[2.1.7. Exchange hexadecimal character string into decimal 6](#_Toc458156298)

[2.2. M1 Card Reader 7](#_Toc458156299)

[2.2.1. Load key into device 7](#_Toc458156300)

[2.2.2. Find card 7](#_Toc458156301)

[2.2.3. Authenticate key 7](#_Toc458156302)

[2.2.4. Authenticate the key with inputting password 8](#_Toc458156303)

[2.2.5. Read card 8](#_Toc458156304)

[2.2.6. Write card 9](#_Toc458156305)

[2.3. Contact CPU Card Reader 9](#_Toc458156306)

[2.3.1. Set the contact card seat that to operate 9](#_Toc458156307)

[2.3.2. Set the parameter of the contact card 9](#_Toc458156308)

[2.3.3. Reset Contact Card 10](#_Toc458156309)

[2.3.4. Contact APDU Exchange 10](#_Toc458156310)

[2.4. Contactless CPU Card Reader 11](#_Toc458156311)

[2.4.1. Find Type A card 11](#_Toc458156312)

[2.4.2. Reset Type A card 11](#_Toc458156313)

[2.4.1. Contactless APDU Exchange 11](#_Toc458156314)

[2.4.2. Find Type B card 12](#_Toc458156315)

[2.5. Magnetic Stripe Reader 12](#_Toc458156316)

[2.5.1. Read data 12](#_Toc458156317)

[2.6. Ultra-Light Card Reader 12](#_Toc458156318)

[2.6.1. Find Ultra-Light card 12](#_Toc458156319)

[2.6.2. Read data 13](#_Toc458156320)

[2.6.3. Write data 13](#_Toc458156321)

[2.7. Ultra-Light C Card Reader 14](#_Toc458156322)

[2.7.1. Find Ultra-Light C card 14](#_Toc458156323)

[2.7.2. Authenticate the key 14](#_Toc458156324)

[2.7.3. Update the key 14](#_Toc458156325)

[2.7.4. Read data 15](#_Toc458156326)

[2.7.5. Write date 15](#_Toc458156327)

[2.8. MIFARE Plus Reader 15](#_Toc458156328)

[2.8.1. Level 0 Function 15](#_Toc458156329)

[2.8.2. Level 1Function 16](#_Toc458156330)

[2.8.3. Level 2 Function 17](#_Toc458156331)

[2.8.4. Level 3 Function 17](#_Toc458156332)

[Appendix ⅠError Code 21](#_Toc458156333)

# Introduction

This document defines the application program interface of Z90 Contact IC Card Reader, including contact CPU reader/writer, 4442 reader/writer, 4428 reader/writer, 24c series reader/writer.

# Application Program Interface

## Device Function

### Initialize the port

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**\* Description:** Initialize the port.

**\* Input:** port: the communication port,

e.g. 100 \\ USB

0 [\\ COM1](file:///\\COM1)

1 \\ COM2

3 \\ COM3

baud: the baud of the device (9600 ~ 115200)

**\* Output:** None

**\* Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

HANDLE IC\_InitComm\_Baud (IN int16 port, IN unsigned long baud);

### Close the port

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Close the port.

\***Input:** icdev: the communicate identifier of the device

\***Output:** None

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ExitComm ( IN HANDLE icdev);

### Beep

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Beep

\***Input:** icdev: the communication identifier of the device

\_Msec: the time of the device beep

e. g.: 10

\***Output:** None

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_DevBeep (IN HANDLE icdev, IN unsigned char \_Msec);

### Read version of the hardware

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** read the version of the hardware.

\***Input:** icdev: the communication identifier of the cevice

\*\_ver: version information

\***Output:** None

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadVer (IN HANDLE icdev, IN unsigned char \*\_ver);

### Write data into memory of the device

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data into memory of the device.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\_data: the data which will be written.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteDevice (IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_data);

### Read data from memory of the device

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read data from memory of the device.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the reading data

\***Output:** \_data: the reading data

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadDevice (IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_data);

### Judge whether there is a card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** 0 [\\ card](file:///\\card) inserted

1 \\ no card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Status (IN HANDLE icdev);

### Test card type

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Test card type.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** 1 \\ AT88SC102

2 \\ AT88SC1604

3 \\ AT88SC1604B

4 \\ AT88SC153

5 \\ AT88SC1608

6 \\ SLE4406

7 \\ SLE4404

8 \\ SLE4442

9 \\ SLE4428

11 \\ AT45D041

12 \\ SSF1101

21 \\ AT24C01A

22 \\ AT24C02

23 \\ AT24C04

24 \\ AT24C08

25 \\ AT24C16

26 \\ AT24C64

30 \\ CPU (T = 0)

31 \\ CPU (T = 1)

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckCard (IN HANDLE icdev);

### Exchange the byte data into string

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Exchange the byte data into string.

\***Input:** strasc: the data which will be exchanged

\_len: the length of the strasc

\***Output:** strhex: the data has been exchanged

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short asc2hex (IN unsigned char \*strasc, OUT unsigned char \*strhex, IN int16 \_len);

### Exchange the string into byte data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Exchange the string into byte.

\***Input:** strhex: the data which will be exchanged

\_len: the length of the strhex

\***Output:** strasc: the data has been exchanged

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short hex2asc (IN unsigned char \*strhex, OUT unsigned char \*strasc, IN int16 \_len);

## 4442 & 4432 Card

### Read protection address

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read protection address.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\***Output:** DataBuffer: the data has been read

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadProtection (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

**Related Function:**

short IC\_ReadProtection\_Hex (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

### Write protection address

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write protection address.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\***Output:** DataBuffer: the data has been written

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteProtection (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

**Related Function:**

short IC\_WriteProtection\_Hex (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

### Read mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read mistakes count.

\***Input:** icdev: the communication identifier of the device

\***Output:**NONE

\***Return:** =0 \\ error

>0 \\ the mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadCount\_SLE4442 (IN HANDLE icdev);

### Verify the password of card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password of card.

\***Input:** icdev: the communication identifier of the device

\_password: the password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckPass\_SLE4442 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckPass\_SLE4442 (IN HANDLE icdev, IN unsigned char \*\_password);

### Modify the password of card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the password of card.

\***Input:** icdev: the communication identifier of the device

\_password: the new password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangePass\_SLE4442 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_ChangePass\_SLE4442 (IN HANDLE icdev, IN unsigned char \*\_password);

### Judge whether there is a 4442 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 4442 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** 0 \\ 4442 inserted

Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_4442 (IN HANDLE icdev);

### Read password of 4442

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read password of 4442.

\***Input:** icdev: the communication identifier of the device

\***Output:** \_password: the password which will be read

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadPass\_SLE4442 (IN HANDLE icdev, OUT unsigned char \*\_password);

**Related Function:**

short IC\_ReadPass\_SLE4442 (IN HANDLE icdev, OUT unsigned char \*\_password);

## 4418 & 4428 Card

### Read protection address

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read protection address.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\***Output:** DataBuffer: the data buffer. The buffer includes two parts. The first part is the card data. The second part is protection flag. It means the data is protected when the value is 0. If the value is 1, the data is unprotected.

\***Return:** < 0 \\ error

>= 0 \\ the length of the effective data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadWithProtection (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

**Related Function:**

short IC\_ReadWithProtection\_Hex (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

### Write card with setting protection

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write card with setting protection.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\***Output:** DataBuffer: the data buffer. The buffer includes two parts. The first part is the card data. The second part is protection flag. It means the data is protected when the value is 0. If the value is 1, the data is unprotected.

\***Return:** < 0 \\ error

>= 0 \\ the length of the protection data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteWithProtection (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

**Related Function:**

short IC\_WriteWithProtection\_Hex (IN HANDLE icdev, IN int16 offset, IN int16 \_len, OUT unsigned char \*DataBuffer);

### Read mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read mistakes count.

\***Input:** icdev: the communication identifier of the device

\***Output:**NONE

\***Return:** =0 \\ error

>0 \\ the mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadCount\_SLE4428 (IN HANDLE icdev);

### Verify the password of card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password of card.

\***Input:** icdev: the communication identifier of the device

\_password: the password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckPass\_SLE4428 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckPass\_SLE4428 (IN HANDLE icdev, IN unsigned char \*\_password);

### Modify the password of card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the password of card.

\***Input:** icdev: the communication identifier of the device

\_password: the new password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangePass\_SLE4428 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_ChangePass\_SLE4428 (IN HANDLE icdev, IN unsigned char \*\_password);

### Judge whether there is a 4428 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 4428 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** 0 \\ 4442 inserted

Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_4428 (IN HANDLE icdev);

## 101 & 102 & 103 Card

### Verify the password of the 102 card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password of the 102 card.

\***Input:** icdev: the communication identifier of the device

\_password: the password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckPass\_102 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckPass\_102 (IN HANDLE icdev, IN unsigned char \*\_password);

### Modify the password of the 102 card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the password of the 102 card.

\***Input:** icdev: the communication identifier of the device

\_password: the new password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangePass\_102 (IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_ChangePass\_102 (IN HANDLE icdev, IN unsigned char \*\_password);

### Read mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read mistakes count.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** =0 \\ error

>0 \\ the mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadCount\_102 (IN HANDLE icdev);

### Erase data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Erase data.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Erase\_102 (IN HANDLE icdev, IN int16 \_offset, IN int16 \_len);

### Verify the key of the user zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the key of the user zone. If verify correctly, all the data in this zone will be set as “FF”.

\***Input:** icdev: the communication identifier of the device

\_snr: number of the user zone

\_password: the password of the user zone

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckAZPass\_102(IN HANDLE icdev, IN int16 \_snr, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckAZPass\_102hex(IN HANDLE icdev, IN int16 \_snr, IN unsigned char \*\_password);

### Modify the key of the user zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the key of the user zone.

\***Input:** icdev: the communication identifier of the device

\_snr: number of the user zone

\_password: the password of the user zone

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangeAZPass\_102(IN HANDLE icdev, IN int16 \_snr, IN unsigned char \*\_password);

**Related Function:**

short IC\_ChangeAZPass\_102hex(IN HANDLE icdev, IN int16 \_snr, IN unsigned char \*\_password);

### Fusing operation

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Fusing operation.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Fuse\_102(IN HANDLE icdev);

### Judge whether there is a 102 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 102 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_102(IN HANDLE icdev);

## 4406 Card

### Read value

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read the value of the 4406 card.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** >= 0 the value of the card

< 0, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_RValue(IN HANDLE icdev);

### Decrease value

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Decrease the value of the 4406 card.

\***Input:** icdev: the communication identifier of the device

\_value: the value which will be decreased

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_RValue(IN HANDLE icdev, IN int16 \_value);

### Erase data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Erase data.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Erase\_4406(IN HANDLE icdev, IN unsigned char \_offset);

### Verify the password of the 4406 card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password of the 4406 card.

\***Input:** icdev: the communication identifier of the device

\_password: password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckPass\_4406(IN HANDLE icdev, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckPass\_4406hex(IN HANDLE icdev, IN unsigned char \*\_password);

### Judge whether there is a 4406 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 4406 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_4406(IN HANDLE icdev);

## 1604 & 1604B Card

### Verify the password of the 1604 or 1604B

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password of the 1604 or 1604B.

\***Input:** icdev: the communication identifier of the device

\_type: the key type

e.g.: 0 \\ all the key

1 \\ the key of the zone 1

2 \\ the key of the zone 2

3 \\ the key of the zone 3

4 \\ the key of the zone 4

11 \\ the wipe key of the zone 1

12 \\ the wipe key of the zone 2

13 \\ the wipe key of the zone 3

14 \\ the wipe key of the zone 4

\_password: the password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckPass\_1604(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

short IC\_CheckPass\_1604B(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

**Related Function:**

short IC\_CheckPass\_1604hex(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

short IC\_CheckPass\_1604Bhex(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

### Modify the password of 1604 or 1604B

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the password of the 1604 or 1604B.

\***Input:** icdev: the communication identifier of the device

\_type: the key type

e.g.: 0 \\ all the key

1 \\ the key of the zone 1

2 \\ the key of the zone 2

3 \\ the key of the zone 3

4 \\ the key of the zone 4

11 \\ the wipe key of the zone 1

12 \\ the wipe key of the zone 2

13 \\ the wipe key of the zone 3

14 \\ the wipe key of the zone 4

\_password: the password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangePass\_1604(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

**Related Function:**

short IC\_ChangePass\_1604hex(IN HANDLE icdev, IN int16 \_type, IN unsigned char \*\_password);

### Read mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read mistakes count.

\***Input:** icdev: the communication identifier of the device

\_type: the type of the count

e.g.: 0 \\ all the key mistakes count

1 \\ the key mistakes count of the zone 1

2 \\ the key mistakes count of the zone 2 (It is only for 1604B)

3 \\ the key mistakes count of the zone 3 (It is only for 1604B)

4 \\ the key mistakes count of the zone 4 (It is only for 1604B)

11 \\ the wipe key mistakes count of the zone 1

12 \\ the wipe key mistakes count of the zone 2

13 \\ the wipe key mistakes count of the zone 3

14 \\ the wipe key mistakes count of the zone 4

\***Output:** NONE

\***Return:** =0 \\ error

>0 \\ the mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadCount\_1604 (IN HANDLE icdev, IN int16 \_type);

### Fusing operation

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Fusing operation.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Fuse\_1604(IN HANDLE icdev);

### Judge whether there is a 1604 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 1604 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_1604(IN HANDLE icdev);

## 24C Series Card

### Write data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data into the card.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\_databuffer: the data which will be written

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Write24(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

**Relative Function:**

short IC\_Write24\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

### Judge whether there is a 24C card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 24C card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_24C02(IN HANDLE icdev);

short IC\_Check\_24C04(IN HANDLE icdev);

short IC\_Check\_24C08(IN HANDLE icdev);

short IC\_Check\_24C016(IN HANDLE icdev);

## 24C64 Card

### Write data into the 24C64 card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data into the 24C64 card.

\***Input:** icdev: the communication identifier of the device

\_offset: offset address

\_len: the length of the data

\_databuffer: the data which will be written

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Write64(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

**Relative Function:**

short IC\_Write64\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

### Judge whether there is a 24C64 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 24C64 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_24C64(IN HANDLE icdev);

## 45DB041 Card

### Read data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read data.

\***Input:** icdev: the communication identifier of the device

\_page: the page of the data

\_offset: offset address

\_len: the length of the data

\***Output:** \_buffer: the reading data

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_DirectRead(IN HANDLE icdev, IN in16 \_page, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_buffer);

**Relative Function:**

short IC\_DirectRead\_Hex(IN HANDLE icdev, IN in16 \_page, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_buffer);

### Write data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data.

\***Input:** icdev: the communication identifier of the device

\_page: the page of the data

\_offset: offset address

\_len: the length of the data

\_buffer: the reading data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_DirectWrite(IN HANDLE icdev, IN in16 \_page, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_buffer);

**Relative Function:**

short IC\_DirectWrite\_Hex(IN HANDLE icdev, IN in16 \_page, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_buffer);

### Judge whether there is a 45DB041 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 45DB041 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_45DB041(IN HANDLE icdev);

## Contact CPU

### Reset contact CPU

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Reset contact CPU.

\***Input:** icdev: the communication identifier of the device

\***Output:** \_len: the length of the reset information

\_redata: the reset information

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CpuReset(IN HANDLE icdev, OUT unsigned char \*\_len, OUT unsigned char \*\_redata);

**Relative Function:**

short IC\_CpuReset(IN HANDLE icdev, OUT unsigned char \*\_len, OUT unsigned char \*\_redata);

### Exchange APDU information

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Exchange APDU information.

\***Input:** icdev: the communication identifier of the device

\_slen: the length of the sending data

\_sendata: the command data

\***Output:** \_rlen: the length of the reset information

\_recdata: the reset information

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CpuApdu(IN HANDLE icdev, IN unsigned char slen, IN unsigned char \*sedata, OUT unsigned char \*\_elen, OUT unsigned char \*\_redcata);

**Relative Function:**

short IC\_CpuApdu\_Hex(IN HANDLE icdev, IN unsigned char slen, IN unsigned char \*sedata, OUT unsigned char \*\_elen, OUT unsigned char \*\_redcata);

### Get protocol of the card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Get protocol of the card.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** < 0 \\ Error code, see Appendix Ⅰ

= 0 \\ T= 0

= 1 \\ T= 1

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CpuGetProtocol(IN HANDLE icdev);

### Judge whether there is a contact CPU inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a contact CPU inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** < 0 \\ Error code, see Appendix Ⅰ

= 0 \\ CPU protocol: T= 0

= 1 \\ CPU protocol: T= 1

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_CPU(IN HANDLE icdev);

### Set parameter of the card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Set parameter of the card. The acquiescent parameter is T = 0, baud = 9600.

\***Input:** icdev: the communication identifier of the device

­\_cputype: card slot type.

e.g.: 12 \\ master card slot

13 \\ SAM1 card slot

14 \\ SAM2 card slot

15 \\ SAM3 card slot

\_cpupro: protocol of the card.

= 0 \\ T = 0; = 1 \\ T = 1

\_cpuetu: delay parameter. If the card’s baud rate is 9600, set this parameter as 92. If the card’s baud rate is 38400, set this parameter as 20.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_SetCpuPara(IN HANDLE icdev, IN unsigned char \_sputype, IN unsigned char \_cpupro, IN unsigned char \_cpuetu);

## 1608 & 153 Card

### Set user zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Set the user zone which will be operated.

\***Input:** icdev: the communication identifier of the device

­\_zone: the number of the user zone

1608: 0 ~ 7

153: 0 ~ 3

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_SetUserZone(IN HANDLE icdev, IN unsigned char \_zone);

### Read user zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read data of the user zone.

\***Input:** icdev: the communication identifier of the device

­\_offset: offset address

\_len: the length of the data

\***Output:** \_databuffer: the read data

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadUserZone(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_databuffer);

**Relative Function:**

short IC\_ReadUserZone\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_databuffer);

### Read config zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read data of the config zone.

\***Input:** icdev: the communication identifier of the device

­\_offset: offset address

\_len: the length of the data

\***Output:** \_databuffer: the read data

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadConfigZone(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_databuffer);

**Relative Function:**

short IC\_ReadConfigZone\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, OUT unsigned char \*\_databuffer);

### Write user zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data into the user zone.

\***Input:** icdev: the communication identifier of the device

­\_offset: offset address

\_len: the length of the data

\_databuffer: the read data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteUserZone(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

**Relative Function:**

short IC\_WriteUserZone\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

### Write config zone

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data into the config zone.

\***Input:** icdev: the communication identifier of the device

­\_offset: offset address

\_len: the length of the data

\_databuffer: the read data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteConfigZone(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

**Relative Function:**

short IC\_WriteConfigZone\_Hex(IN HANDLE icdev, IN int16 \_offset, IN int16 \_len, IN unsigned char \*\_databuffer);

### Read fuse

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read fuse.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅱ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadFuse(IN HANDLE icdev);

### Write fuse

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write fuse.

\***Input:** icdev: the communication identifier of the device

\_fusetype: set as 0

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteFuse(IN HANDLE icdev, IN unsigned char \_fusetype);

### Verify reading password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the reading password.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\_pass: the password which will be verified

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckRPassword(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

**Relative Function:**

short IC\_CheckRPassword\_Hex(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

### Verify the writing password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the writing password.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\_pass: the password which will be verified

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckWPassword(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

**Relative Function:**

short IC\_CheckWPassword\_Hex(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

### Modify the reading password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the reading password.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\_pass: the new password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangeRPassword(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

**Relative Function:**

short IC\_ChangeRPassword\_Hex(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

### Modify the writing password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Modify the writing password.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\_pass: the new password

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ChangeWPassword(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

**Relative Function:**

short IC\_ChangeWPassword\_Hex(IN HANDLE icdev, IN unsigned char \_zone, IN unsigned char \*\_pass);

### Read the reading password mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read the reading password mistakes count.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadRPasswordCount(IN HANDLE icdev, IN unsigned char \_zone);

### Read the writing password mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read the writing password mistakes count.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadWPasswordCount(IN HANDLE icdev, IN unsigned char \_zone);

### Read the authentication mistakes count

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read the authentication mistakes count.

\***Input:** icdev: the communication identifier of the device

\_zone: the number of the key zone, for the 1608, this value ranges from 0 to 7; for 153, this value ranges from 0 to 1.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadAuthCount(IN HANDLE icdev, IN unsigned char \_zone);

### Initialization authentication

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Initialization authentication. Write the random number into the card.

\***Input:** icdev: the communication identifier of the device

\_num: the random number.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_InitAuth(IN HANDLE icdev, IN unsigned char \*\_num);

**Relative Function:**

short IC\_InitAuth\_Hex(IN HANDLE icdev, IN unsigned char \*\_num);

### Card authenticates the mainframe

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Card authentications the mainframe.

\***Input:** icdev: the communication identifier of the device

\_Q1: the authentication data.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CheckAuth(IN HANDLE icdev, IN unsigned char \*\_Q1);

**Relative Function:**

short IC\_CheckAuth\_Hex(IN HANDLE icdev, IN unsigned char \*\_Q1);

### Mainframe authentication initialization

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Mainframe authentication initialization.

\***Input:** \_Ci: authentication number

\_Gc: the password key

\_Q0: the random number.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short SetInit(IN unsigned char \*\_Ci, IN unsigned char \*\_Gc, IN unsigned char \*\_Q0);

**Relative Function:**

short SetInit\_Hex(IN unsigned char \*\_Ci, IN unsigned char \*\_Gc, IN unsigned char \*\_Q0);

### Mainframe authenticates the card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Mainframe authenticates the card and creates two authentication data.

\***Input:** \_Q1: the one of the two authentication data

\_Q2: the another one of the two authentication data.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short Authenticate(IN unsigned char \*\_Q1, IN unsigned char \*\_Q2);

**Relative Function:**

short Authecticate \_Hex(IN unsigned char \*\_Q1, IN unsigned char \*\_Q2);

### Judge whether there is a 1608 card inserted

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Judge whether there is a 1608 card inserted.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Check\_1608(IN HANDLE icdev);

## RF Card

### RF module reset

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** RF module reset.

\***Input:** icdev: the communication identifier of the device

\_mesc: reset time, when the value is 0, this function will close the RF module of the device.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ResetMifare(IN HANDLE icdev, IN \_int16 \_msec);

### Find card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Find card.

\***Input:** icdev: the communication identifier of the device

\_mode: the mode of finding card, the value 0 is for IDLE and the value 1 is for ALL.

\***Output:** \_snr: the serial number of the card

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Card(IN HANDLE icdev, IN unsigned char \_mode, OUT unsigned char \*\_snr);

**Relative Function:**

short IC\_Card \_Hex(IN HANDLE icdev, IN unsigned char \_mode, OUT unsigned char \*\_snrstr);

### Stop operating current card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Stop operating current card.

\***Input:** icdev: the communication identifier of the device

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Halt(IN HANDLE icdev);

### Load key of the M1

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Load key of the M1.

\***Input:** icdev: the communication identifier of the device

\_mode: the mode of the key, the value 0 is for KEYA of KEYSET0, the value 4 is for KEYB of KEYSET0.

\_secNr: the number of sector

\_key: the password data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Load\_Key(IN HANDLE icdev, IN BYTE \_mode, IN BYTE \_secNr, INT unsigned char \*\_key);

**Relative Function:**

short IC\_Load\_Keyhex(IN HANDLE icdev, IN BYTE \_mode, IN BYTE \_secNr, INT unsigned char \*\_keystr);

### Verify the password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the password.

\***Input:** icdev: the communication identifier of the device

\_mode: the mode of the key, the value 0 is for KEYA of KEYSET0, the value 4 is for KEYB of KEYSET0.

\_secNr: the number of sector

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Authentication(IN HANDLE icdev, IN BYTE \_mode, IN BYTE \_secNr);

### Read data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read data from a appointed block.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 0 to 63

\***Output:** \_data\_buff: the read data

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadMifare(IN HANDLE icdev, IN BYTE \_addr, OUT BYTE \*\_data\_buff);

**Relative Function:**

short IC\_ReadMifare\_Hex(IN HANDLE icdev, IN BYTE \_addr, OUT BYTE \*\_data\_buff);

### Write data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Write data from a appointed block.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 0 to 63

\_data\_buff: the written data whose length is 16 bytes

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_WriteMifare(IN HANDLE icdev, IN BYTE \_addr, IN BYTE \*\_data\_buff);

**Relative Function:**

short IC\_WriteMifare\_Hex(IN HANDLE icdev, IN BYTE \_addr, IN BYTE \*\_data\_buff);

### Initialize the value into 0

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Initialize the value into 0.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 1 to 63

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Init\_Value(IN HANDLE icdev, IN BYTE \_addr);

### Read value

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read value.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 1 to 63

\***Output:** \_value: the read value

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Read\_Value(IN HANDLE icdev, IN BYTE \_addr, OUT long \*\_value);

### Increase value

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Increase value.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 1 to 63

\_value: the value which will be increased

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Increment(IN HANDLE icdev, IN BYTE \_addr, IN DWORD \_value);

### Decrease value

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Decrease value.

\***Input:** icdev: the communication identifier of the device

\_addr: the block address which ranges from 1 to 63

\_value: the value which will be decreased

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Decrement(IN HANDLE icdev, IN BYTE \_addr, IN DWORD \_value);

### Verify the key with the password data

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Verify the key with the password data.

\***Input:** icdev: the communication identifier of the device

\_mode: the mode of the key, the value 0 is for KEYA of KEYSET0, the value 4 is for KEYB of KEYSET0.

\_addr: the address number of the key block

\_passbuff: the password data

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Authentication\_Passaddr(IN HANDLE icdev, IN unsigned char \_mode, IN unsigned char \_

addr, IN unsigned char \*\_passbuff);

**Relative Function:**

short IC\_Authentication\_Passaddrhex(IN HANDLE icdev, IN unsigned char \_mode, IN unsigned char \_addr, IN unsigned char \*\_passbuff);

## ISO-144443-4 Protocol Card

### Set the card type which will be operated

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Set the card type which will be operated.

\***Input:** icdev: the communication identifier of the device

\_type: the card type , the value ‘A’ is for TypeA, the value ‘B’ is for TypeB.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Config\_Card(IN HANDLE icdev, IN unsigned char \_type);

### RF reset function

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** RF reset function, this function is only for TypeA.

\***Input:** icdev: the communication identifier of the device

\***Output:** \_len: the length of the reset information

\_recbuff: the reset information

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Pro\_Reset(IN HANDLE icdev, OUT unsigned char \*\_len, OUT unsigned char \*\_recbuff);

**Relative Function:**

short IC\_Pro\_Resethex(IN HANDLE icdev, OUT unsigned char \*\_len, OUT unsigned char \*\_recbuff);

### Exchange APDU

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Exchange APDU.

\***Input:** icdev: the communication identifier of the device

\_slen: the length of the sending APDU

\_sdata: the APDU data

\_timeout: delay time

\_FG: the length of segmentation and this value should be smaller than 64.

\***Output:** \_rlen: the length of the response information

\_rdata: the response information

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Pro\_Commandlink(IN HANDLE icdev, IN unsigned char \_slen, IN unsigned char \*sdata, OUT unsigned char \*\_rlen, OUT unsigned char \*\_rdata, IN unsigned char \_timeout , IN unsigned char FG);

**Relative Function:**

short IC\_Pro\_Commandlinkhex(IN HANDLE icdev, IN unsigned char \_slen, IN unsigned char \*sdata, OUT unsigned char \*\_rlen, OUT unsigned char \*\_rdata, IN unsigned char \_timeout , IN unsigned char FG);

### Find TypeB

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Find TypeB.

\***Input:** icdev: the communication identifier of the device

\_mode: set as 0

\_AFI: the parameter of anti-collision

\_N: identifier of the application cluster.

\***Output:** \_ATQB: the returning information

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Request\_B(IN HANDLE icdev, IN unsigned char \_mode, IN unsigned char \_AFI, IN unsigned char \_N, OUT unsigned char \*\_ATQB);

**Relative Function:**

short IC\_Request\_Bhex(IN HANDLE icdev, IN unsigned char \_mode, IN unsigned char \_AFI, IN unsigned char \_N, OUT unsigned char \*\_ATQB);

### Active the TypeB

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Active the TypeB.

\***Input:** icdev: the communication identifier of the device

\_PUPI: parameter, refer to 14443-3

\_CID: the value ranges from 0 to 14.

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_Attrib(IN HANDLE icdev, IN unsigned char \*\_PUPI, IN unsigned char \_CDI);

**Relative Function:**

short IC\_Attrib\_Hex(IN HANDLE icdev, IN unsigned char \*\_PUPI, IN unsigned char \_CDI);

## LCD Operation

### Display specific buffer on the LCD

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Display specific buffer on the LCD.

\***Input:** icdev: the communication identifier of the device

\_line: number of the line which will show the specific buffer

\_offset: offset address.

\_strData: the specific buffer which will be showed

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_DispInfo(IN HANDLE icdev, IN unsigned char \_line, IN unsigned char \_offset, IN char \*strData);

### Display system information on the LCD

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Display system information on the LCD.

\***Input:** icdev: the communication identifier of the device

\_flag: information identifier:

1 // display “insert card”

3 // display “present card”

4 // display “operation failed”

5 // display “enter password”

6 // display “password error”

7 // display “succeeded”

9 // display “error”

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_DispLcd(IN HANDLE icdev, IN unsigned char \_flag);

### LCD backlight control

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** LCD backlight control.

\***Input:** icdev: the communication identifier of the device

\_flag: the control flag, the value 1 is for opening LCD backlight; the value 0 is for closing LCD backlight

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_CtlBackLight (IN HANDLE icdev, IN unsigned char \_flag);

### Clear the LCD

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Clear the LCD.

\***Input:** icdev: the communication identifier of the device

\_line: the value stands for how many lines you want to clear

\***Output:** NONE

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_LcdClrScrn(IN HANDLE icdev, IN unsigned char \_line);

## Keyboard operation

### Get the inputting password

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Get the inputting password.

\***Input:** icdev: the communication identifier of the device

\_ctime: delay time

\***Output:** \_rlen: the length of the inputting password

\_cpass: the inputting password

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_GetInputpss(IN HANDLE icdev, IN unsigned char \_ctime, OUT unsigned char \*\_rlen, OUT unsigned char \*\_cpass);

## Magnetic Card

### Read track data from the magnetic card

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\***Description:** Read track data from the magnetic card.

\***Input:** icdev: the communication identifier of the device

\_ctime: delay time

\***Output:** \_Track1Data: the data of the track 1

\_Track1Len: the length of the data which was read from track 1

\_Track2Data: the data of the track 2

\_Track2Len: the length of the data which was read from track 2

\_Track3Data: the data of the track 3

\_Track3Len: the length of the data which was read from track 3

\***Return:** Error code, see Appendix Ⅰ

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

short IC\_ReadMagCardAll(IN HANDLE icdev, IN unsigned char \_ctime, OUT unsigned char \*\_Track1Data, OUT unsigned long \*\_Track1Len, OUT unsigned char \*\_Track2Data, OUT unsigned long \*\_Track2Len, OUT unsigned char \*\_Track3Data, OUT unsigned long \*\_Track3Len);

# Appendix ⅠError Code

|  |  |
| --- | --- |
| Code Value | Description |
| 0 | Operation Success |
| -39 | Communication error |
| -2 | Can’t support the function |
| -3 | Card type error |
| -32 | Open port error |
| -33 | Get the status of the port error |
| -34 | Set the status of the port error |
| -35 | Close the port error |
| -36 | The port is initialized |
| -128 | Reading error |
| -129 | Writing error |
| -130 | Authentication error |
| -132 | Time out |
| -134 | No card |
| -135 | The format of the parameter of the function is illegal |

# Appendix ⅡError Code

|  |  |
| --- | --- |
| Code Value | Description |
| < 0 | Error, see Appendix Ⅰ |
| >= 0 | Correct, see Value Table |

**Value Table**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| BIT7 | BIT6 | BIT5 | BIT4 | BIT3 | BIT2 | BIT1 | BIT0 |
| 0 | 0 | 0 | 0 | 0 | PER | CMA | FAB |